GPS INTERNAL PASSIVE ANTENNA
N. Navarro – 3/14/2008

Material:  22 AWG pre-tinned, insulated stranded wire. Brown colored
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                                             SOLDER THE STRIPPED END OF WIRE TO PIN 1 OF ANTENNA PADS
